

**How to Pressure Check Tubes/Find Leaks
Paddle Boat Tubes**

1. Drain any water from the tube by drilling a hole in the bottom of the butt cap using a small drill bit (1/16”). Let all the water drain out. Weld the hole closed.

Soap Formula

* 3 Tablespoons Full of Dollar General Baby Shampoo (13.6 fl oz)
* ½ Gallon of Water
1. Combine the ingredients above and shake well in a spray bottle.
2. Spray the entire tube and welds with the soapy water mix.
3. Take the screw with the o-ring off, located at the top of the tube in the back.
4. Put air in the tube for around 4-6 seconds or 4-6 pounds.

Put thumb over where the screw was and check for bubbles and/or a hissing sound. Any hole found should be welded and re-pressure tested.