New Lo Pro Canopy Rail Bracket Mounts

1. Measure 7” from the backside of the rear wall to the center of the pin hole on the mounting bracket to place the rear bracket.
2. Drill the bracket to the frame from the pre-drilled holes that are already in the bracket and screw it down.
3. Measure 28 5/8” forward to the center of the pin hole for the middle bracket.
4. Drill the bracket to the frame from the pre-drilled holes that are already in the bracket and screw it down.
5. Measure 27 7/8” forward to the center of the pin hole for the front bracket.
6. Drill the bracket to the frame from the pre-drilled holes that are already in the bracket and screw it down.
7. The two bigger pins will be for the rear brackets that are drilled to 5/16”.

The two smaller pins are for the middle and front brackets depending on the positioning of the canopy.

The two bigger pins are for the rear brackets that are drilled to 5/16”.

Note: If you are having troubles getting the rear pin in the hole, drill the hole with a 5/16” bit to widen it for a better fit.