CANOPY MOUNTING BRACKETS FOR A LO PRO

* Measure 7 ¾” from the backside of the rear wall to the center of the pin hole on the mounting bracket to place the rear bracket
* Drill the bracket to the frame from the pre-drilled holes that are already in the bracket
* Measure 28 5/8” forward to the center of the pin hole for the middle bracket
* Drill the bracket to the frame from the pre-drilled holes that are already in the bracket
* Measure 24 15/16” forward to the center of the pin hole for the front bracket
* Drill the bracket to the frame from the pre-drilled holes that are already in the bracket
* The two bigger pins will be for the rear brackets that are drilled to 5/16”
* The two smaller pins are for the middle and front brackets depending on the positioning of the canopy

Note: If you are having troubles getting the rear pin in the hole, drill the hole with a 5/16” bit to widen it for a better fit.