Canopy Positioning

\*\*\*It is important to have one person on each side of the Lo Pro to move the canopy together. This is a two-person task.

How to Position the Canopy for Trailering:

1. Unhook the support straps from the front railing hooks.
2. Push the front of the canopy back until it is folded up.
3. Put the canopy boot on the canvas.
4. Unpin the rear support bracket arms while holding on to the middle support arms.
5. Unpin the middle canopy arms and gently move the canopy forward on both sides until you reach the front brackets.
6. Pin the main canopy arms to the front brackets and gently walk the canopy back until it lays nicely on the railing.
7. This puts the canopy in the trailering position.

How to Open the Canopy:

1. Make sure the main canopy arms are pinned in the middle brackets and the support arms are pinned in the rear brackets.
2. Take off the boot by unzipping it from the canopy.
3. Grab the front bow and pull it forward until the canopy is completely open.
4. Hook the straps from the front bow loop to the loop that is on the railing of the boat by the front bracket.
5. Tighten the straps to create tension by pulling the front bow forward slightly.

How to Close the Canopy

1. The main canopy arms should be in the middle brackets and the support arms should be in the rear brackets.
2. Unhook the straps from the railing hooks on each side.
3. Push the front bow back until the canopy is folded up.
4. Put the boot on the canopy and zip it up.